---
name: Bug report
about: Create a report to help us improve
title: ''
labels: ''
assignees: ''

---

### Describe the bug
*Please describe what you observe on the display or any error messages*

### Device hardware
- *MCU*: ??? ATmega2560, ESP32, etc.
- *Display with link*: ??? Adafruit ILI9341 2.8" resistive (https://www.adafruit.com/product/1651)
- *GUIslice config selected*: ??? `ard-adagfx-ili9341-stmpe610`

### Checklist to try first
*Most display/touch issues can be identified by working through the steps in the [Configuring GUIslice](https://github.com/ImpulseAdventure/GUIslice/wiki/Configuring-GUIslice) guide.*

*Please confirm whether:*
- *Display works correctly with standalone display driver library examples (eg. TFT_eSPI graphicstest, Adafruit graphicstest, etc.) without GUIslice:* ???
- *Touch works correctly with standalone touch library examples without GUIslice:* ???

### Expected behavior
*A description of what you expected to happen*

### Initialization messages
*Please copy any startup messages / errors reported to the serial monitor window here. You can enable all error messages by setting `DEBUG_ERR 2` in the GUIslice config file.*

### Additional info
*Add any other context about the problem here.*
